

CM1 CATAMARAN Setup Guide (Desktop)


1. Navigate to <http://gps.shipcomwireless.com/downloads/vacm1.html> to download the CATAMARAN Client software.




1. Choose the option “CATAMARAN Client software for Windows Desktop/Laptop” and save the DesktopClient.zip.
2. Navigate to the save file location and right click the zip file, DesktopClient.zip. Select “extract all” to unzip the file. (Zip Password: Shipcom2016)
3. Open the resultant “DesktopClient” folder




1. (Optional) To create a shortcut of the executable, right click on CM001FDN.exe. Select create shortcut, then drag the shortcut to the desktop.
2. Open CM001FDN.exe (or the shortcut if created in the previous step). If the “Open File – Security Warning” appears, click Run.




1. Click Tools -> Options




1. Enter the Server URL given by your system administrator
2. Check the “Enable Offline” checkbox
3. Click the “Local” link and select a location for the offline database to be saved (It is recommended to create a new folder to contain the database)
4. Click “Apply”
5. Enter credentials provided and log into CATAMARAN



1. On the menu, click “Request Access”



1. Click the “Provision” button



1. Input a description of your device
2. Ensure “Reprovision” is checked
3. Select a cemetery that you want to associate your device to from the dropdown
4. Click the “Provision” button
5. From the main menu, click Tools -> Sync
6. After sync is completed wait for a minimum of 2 minutes
7. After 2 minutes you will have to sync one more time, click Tools -> Sync
8. Your device is now setup for CATAMARAN and can now be used.